MIDI configuration

This panel is used to configure the MIDI interfaces.

Setting | Description
Input device | Selects a MIDI input device to control the pattern editor.
Output device | Output commands to a MIDI device.
Master sync | Generates ticks.
Do not record key releases | Skip recording of key release commands.
Map MIDI to NES channels | Maps the MIDI channels to the tracker channels (MIDI channel 0 = square 1, channel 1 = square 2...)
Record velocities | Translate MIDI note velocities to a volume value.
Auto arpeggiate chords | Arpeggiate multiple keypresses.

Back to configuration · interface · main index