Sound configuration

This panel is used to configure the audio settings.

Setting | Description
Device | The DirectSound device used for audio output.
Sample rate | Audio sample rate, should be set to the native setting of your sound card.1
Sample size | Audio sample size, use 16 unless you are using a really old sound card.
Buffer length | Audio buffer length. Keep as short as possible for lowest delay. (Default: 40 ms)
Bass filtering | Blip-buffer bass filtering, default: 20 Hz.
Treble filtering | Blip-buffer treble filtering, default: 12kHz, -24 dB.
Volume | Sound volume level.

1. This program is using band-limited synthesis, a higher sample rate is not necessary for high audio quality.

Back to configuration · interface · main index