Configuration

The configuration window consists of five categories.
1. General

Wrap cursor | Screen wraps when the cursor has reached the end or top of the pattern.
Free cursor edit | Removes the cursor from the middle of the screen.
Preview wave-files | Preview wave files in the import wave to DPCM open file window.
Key repeat | Enables key repetition.
Show row numbers in hex | Displays the row number in hexadecimal or decimal notation.
Preview next/previous frame | Display the next and previous frame in shaded before the start and after the end of current frame.
Don't reset DPCM on note stop | Removes DPCM popping when keys are released. May decrease the level of triangle and noise as a result of DPCM not being resetted. Press F12 to do it manually.
Ignore step when moving | Ignore the step setting when moving the cursor and only use it when inserting notes
Pattern colors | Display the patterns in colors
Delete-key will pull up rows | Pull up rows below the deleted row

Track edit style

FastTracker II | Step down after an instrument/effect number was entered
Modplug | Stays on the same line after an instrument/effects number was entered
Impulse Tracker | Behaves like Impulse tracker when entering effects.

Page jump length: number of rows to skip when pressing page up/down.
2. Appearance
This section is for customizing the colors. Choose between a few predefined schemes or set up your own.
3. MIDI

Input device | Choose the device from which you want to record MIDI messages.
Output device | Choose a device you want to send MIDI messages to.
Master sync | Making the tracker to step down after each sixth's clock tick.
Do not record key releases | Skip recording of key releases.
Map MIDI to NES channels | Maps MIDI-channel messages to NES-channels, channel 1 will be square 1, channel 2 is square 2 and so on. If not checked, the selected channel in the tracker will receive all messages.
Record velocities | Converts key-velocities into volume levels and stores them in the volume column.
Auto arpeggiate chords | Plays an arpeggio if more than one key are pressed on the MIDI keyboard.

4. Sound

Device | The device that receives the audio
Sample rate | The rate of samples in hertz, default is 44.1 kHz.
Sample size | Size of samples, default is 16 bit. Change only if needed.
Buffer length | The length of the sound buffer, default is 40 ms. Increase if you're experiencing sound problems.
Bass filtering | Sets the bass filtering frequence (also known as a high-pass filter). Default is 16 Hz.
Treble filtering | Sets the treble filtering frequence and cut off strength. Default is -3 dB and 12 000 Hz.
Volume | Volume level

5. Shortcuts
This section allows you to customize the key shortcuts in the program. (Note that the menus will still display the default settings.)