NSF export

NSF (Nintendo Sound Format, invented by Kevin Horton) is a type of file used to represent NES music. To create NSF files, select Create NSF from the File menu to open the NSF export window.

The NSF file options contains some options related to the NSF file format: the song information fields is the same as in the control panel. There is also a system type option: NTSC, PAL or Dual. Select Dual if you want the NSF to be playable on both types of system.

A few other formats beside NSF are also available:

- NSF
  Creates a NSF file.
- NES
  Encapsulates the NSF into a NES file that can be played in emulators or with carts like PowerPak.
- BIN
  Stores only the music data and DPCM samples in separate files, for use with the NSF driver sources which are available from the web page.
- PRG
  Creates a single 32 kB program ROM file, ready to be used with a NROM-compatible cart for playback on NES hardware.
- ASM
  Stores the music data and samples in text format that can be used with the driver sources (for CA65). More flexible than the BIN option.

As of version 0.3.5, an export plugin system has been added that allows exporting to custom formats. New export targets will appear in the drop-down menu when export plugin DLLs are added. More info about this is available on the web page.

Back to interface · main index